STGSM Video Denoising Toolbox 1.0.0
-------------------------------------------------------------------
Last Revision: Feb, 2007

 This toolbox is a  MATLAB realization of the algorithm described in [1].

  [1] G. Varghese and Z. Wang, “Video denoising based on a
      spatiotemporal Gaussian scale mixture model,” IEEE Transactions on 
       Circuit and Systems for Video Technology, to appear, 2010

The toolbox is built on the BLS-GSM toolbox develeoped by Javier Portilla(http://decsai.ugr.es/~javier/denoise/).



INSTALLATION 
-------------------------------------------------------------------

1) Use MATLAB 7.0  or above .

2) Unpack the zip file into a directory in your hard drive.


Using the toolbox
-------------------------------------------------------------------
Refer to video_denoi_demo.m for detailed usage instructions.
The toolbox expects YUV 4:2:0 sequence as inputs, sample sequence is provided along with toolbox.
To add noise to sequence use AddNoiseLuma.m



Please, report all comments and issues to gijesh.varghese@gmail.com.